Smart Home

[Introduction 2](#_Toc36401701)

[Database 2](#_Toc36401702)

[Web Server 4](#_Toc36401703)

[Environment 4](#_Toc36401704)

[Project Management 4](#_Toc36401705)

[Source Code 4](#_Toc36401706)

[Design 5](#_Toc36401707)

[Modules : 5](#_Toc36401708)

[System Manager 5](#_Toc36401709)

[Communication Manager 5](#_Toc36401710)

[Database Manager 11](#_Toc36401711)

[App manager 11](#_Toc36401712)

[Users Manager 11](#_Toc36401713)

[Security 11](#_Toc36401714)

[Quick Startup Guide 11](#_Toc36401715)

[Resources 11](#_Toc36401716)

# Introduction

The objective of this project is to build a generic infrastructure to host a smart home applications.

# Database

Postgresql will be the database used in the projects to store all the program data. For C/C++ applications Postgresql C/C++ Interface API will be used.

sudo apt-get install postgresql

*performing post-bootstrap initialization ... ok*

*syncing data to disk ... ok*

*Success. You can now start the database server using:*

*/usr/lib/postgresql/10/bin/pg\_ctl -D /var/lib/postgresql/10/main -l logfile start*

Use systemctl command to manage postgresql service:

1. stop service:

systemctl stop postgresql

1. start service:

systemctl start postgresql

1. show status of service:

systemctl status postgresql

1. disable service(not auto-start any more)

systemctl disable postgresql

1. enable service postgresql(auto-start)

systemctl enable postgresql

/var/lib/postgresql/10/main

Postgresql version = 10

config files : /etc/postgresql/10/main/

log file : /var/log/postgresql/postgresql-10-main.log

<http://manpages.ubuntu.com/manpages/eoan/en/man1/pg_lsclusters.1.html>

Latest Postgresql C++ client code : <https://github.com/jtv/libpqxx>

Postgresql tutorial : <https://www.tutorialspoint.com/postgresql/postgresql_c_cpp.htm>

psql -U postgres

libtool: finish: PATH="/usr/local/sbin:/usr/local/bin:/usr/sbin:/usr/bin:/sbin:/bin:/usr/games:/usr/local/games:/sbin" ldconfig -n /usr/local/lib

----------------------------------------------------------------------

Libraries have been installed in:

/usr/local/lib

If you ever happen to want to link against installed libraries

in a given directory, LIBDIR, you must either use libtool, and

specify the full pathname of the library, or use the '-LLIBDIR'

flag during linking and do at least one of the following:

- add LIBDIR to the 'LD\_LIBRARY\_PATH' environment variable

during execution

- add LIBDIR to the 'LD\_RUN\_PATH' environment variable

during linking

- use the '-Wl,-rpath -Wl,LIBDIR' linker flag

- have your system administrator add LIBDIR to '/etc/ld.so.conf'

See any operating system documentation about shared libraries for

more information, such as the ld(1) and ld.so(8) manual pages.

----------------------------------------------------------------------

make[2]: Nothing to be done for 'install-data-am'.

# Web Server

Apache Tomcat

# Environment

The entire project will be hosted inside a docker container.

The project image “smarthome” can be downloaded from the below docker hub.

<https://cloud.docker.com/repository/docker/pruthwinkg/dockerhub-pruthwinkg/general>

# Project Management

The project management tool used for this project is “Trello”.

Below is the link of the project management activities for this project.

<https://trello.com/b/OG8rQ0q8/smart-home-system>

# Source Code

The source code of this project is maintained in the “Bitbucket” repository.

<https://bitbucket.org/Pruthwinkg/hobbyprojects/src/master/SmartHome/>

apt-get install libpq-dev

apt-get install libboost-all-dev

# Design

## Modules :

### System Manager

System Manager allocates UIDs for each sub-system. The UIDs can be allocated statically or dynamically. There are 1024 well known static UIDs defined. All the sub-systems required for the smooth functionality and support of the system is allocated a well known UID. Most of the user apps are allocated dynamic UIDs.

The Application Manager which is responsible for handling user apps borrows the dynamic UIDs from the System Manager.

These UIDs are required for Communication Manager during the protocol phase.

Future Request for this module:

- The deletion of clients should be more smarter. There has to be a option to notify the clients, so that the clients can finish and respond back to the sysmgr that they are ready to be deleted. This notification can be sent over SCOM messages with a super priority.

### Communication Manager

<https://opensource.com/article/19/4/interprocess-communication-linux-storage>

<https://opensource.com/article/19/4/interprocess-communication-linux-channels>

<https://opensource.com/article/19/4/interprocess-communication-linux-networking>

This subsystem will handle all kinds of communications (within the system and to outside).

From the articles above, the Unix Domain Sockets (UDS) suits well for this application. The Comm manager will also implement other IPC mechanisms as well incrementally. But the primary mode of communication will be via Unix Domain Sockets.

The comm\_mananger will implement below features :

- Message Queuing

- Priority based message delivery

- Direct channel establishment for bulk data delivery between two modules (Like DMA)

- Backing of messages (in case of restarts/crashes)

- Stream and Datagram support

- Event Handling (Does this has to be handled by a new subsystem, like Event Manager ???)

The UDS Server will always run in the context of comm\_manager. The comm\_mananger will provide a shared library to create clients for each subsystems who wants to participate in the communication. The UDS clients will run in the context of each subsystem.

**Note : Eth and IP header is valid only for communication outside the system**

|  |  |  |  |
| --- | --- | --- | --- |
| Eth | IP | Communication Manager Header | Pay load |

**Communication Manager Protocol:**

Communication Manager is an intelligent module whose main responsibility is to transfer data from process to another. This module supports numerous features. The Communication Manager has two parts i.e, Server Instances and Library part.

Communication Manager uses a custom protocol for reliable data transfer. It has mainly three stages. The protocol is always initiated by the communication manager. It not necessary that all these steps happen sequentially. The Server Instance and the Communication Manager library follows a series of steps before allowing any regular data transmission. The library tries to offload many data storing, so that Communication Manager remains faster. But Communication Manager can still store some data packets if required.

**Discovery Phase**:

Every process will be identified by an UID. (Statically allocated/ Dynamically allocated by System Manager, written to mmap). Discovery phase is usually kick started when an app uses the communication system for the first time. If an app never communicates with anyone, none of the protocol kicks in. During this phase, the Communication Manger discovers that such a process exists in the system and makes a note of it.

The Communication Manager library maintains a state machine to know the Communication state of an app. When an app wants to send messages/data to another app, the Communication Library allows the data to be sent only if the current state of the app is in Data Transfer ready. The library will hold the data in its internal queues and kick starts the protocol by sending a copy of this data packet to the Server Instance.

Upon receiving the data packet from the app for the very first time, the Server Instance will initiate the Discovery protocol. During the discovery phase, the Communication Manager will send a discovery msg to the client, from where it received the message for the very first time. The Communication Manager also sends some system wide information in the Discovery messages for the app to consume. It’s up to the app, to make use of this system wide data.

The client needs to send an ACK for the Discovery message. The client also has to respond back to the Communication Manager with a Discovery message along with its UID.

Now the Communication Manager maintains a map of <UID,Server FD>. This indirectly helps in the Learning phase as well for other apps who wants to send messages to this app.

Now the Communication Manager library of the app will set the state of the app to “Data Transfer Ready” and will send the data packet which was enqueued in its internal queues to the Server Instance. If the destination UID is also discovered by the Server Instance, then the packets are sent. Else, the Server Instance will notify the library to hold off any data packet sending to this particular destination UID, until it is Discovered (Learning phase).

“Data Transfer Ready” doesn’t necessarily mean that the Data packets can reach the destination apps. It just means that the source app is ready for Communication. But it guarantees that it can receive the packets from other apps. Till the Destination app is also Discovered by the Communication Manager, the source app cannot send any data packets to that destination.

The library will make a note that, this particular destination UID is not yet reachable and will start queuing the data packets if the app keeps sending the data packets to this destination. The library can also ask the app to throttle the messages in case lot of messages for this destination starts to build up in its internal queues. The queues are per destination UID.

**Learning:**

The learning phase is indirectly assisted by the Discovery phase. As mentioned in the previous phase, if a destination UID is not yet reachable, the library will stop sending any data packets for this destination to the Communication Manager. Soon after the Discovery phase, when the library sends a data packet again to the Communication Manager, if the destination UID is not learnt/Discovered, the Communication Manager will send a learning message with payload as NULL followed by the destination UID. Once the Destination app is also discovered by the Communication Manager, it will send Learning messages to all those apps who wanted to send data to this destination previously. After the Discovery phase, when an app sends data packets for a destination who is not yet discovered, the Communication Manager will maintain an interest table to know who are interested to send data to this destination.

The learning message is a simple message without requiring any ACK. Upon receiving this learning message, the Communication Manager library will start sending messages which were queued up in its internal queues for this destination. The payload of the learning message will contain the destination UID if that destination has been discovered/learnt by the Communication Manager.

Since the learning message doesn’t require ACK, after sending the learning messages to the interested apps, the Communication manager will clear the interest tables for this destination UID. If an app misses the learning message, then there is no way to notify the app unless the app tries to send the message to the Communication Manager again.

The library can alternatively send a special system message to the Communication Manager asking whether the Destination is learnt/discovered.

**Data Transfer:**

After the source UID and destination UID are both discovered/learnt by the Communication Manager, an app can actually send data to that destination UID. If Communication Manager sends learning message with payload as NULL followed by a destination UID, at any point of time, the clients should hold all its further messages to that destination UID. Else, the Communication Manager drops those messages.

The Communication Manager can simply decide to throttle the messages from a source app, in case if the Communication Manager is extremely loaded OR it receives extreme large quantities of messages from this source app OR if a destination is not yet discovered/learnt. To throttle the messages for a particular destination, it will simply send a learning message with NULL followed by a destination UID in its payload. The client app should stop sending any further messages for any destination till receives again a learning message with destination UID in its payload. The Communication Manager can also send a special system message to indicate the app to stop sending to any destination.

|  |  |
| --- | --- |
| **Message Format** | **Functionality** |
| Protocol | Discovery | <system info> | During discovery phase |
| Protocol | Learning | <NULL, Destination UID> | Destination not learnt. Stop sending to this UID |
| Protocol | Learning | <Destination UID> | Destination learnt. Start sending to this UID |
| ACK | Proto ack/nack | | Acknowledgment for Protocol packets |
| ACK | Data ack/nack | | Acknowledgment for Data packets |
| System | Communication | <msg id> | Refer system messages section for more details about this type of messages.  Depending on msg\_id value, the messages can be throttled for all destinations from this source UID |

The Communication Manager and its library will support APIs to encode and decode messages required for the protocol.

**Multi-Master instances:**

The Communication Manager supports multi-master instances. These are the instances of the Communication Manager, but all of them runs in the context of Communication Manager. There is a software limit of max 5 master instances in a system, due to memory and computing limitations of the underlying hardware on which the system runs. Each Master instances can belong to different AF types or can also create multiple masters of the same AF types. All these Master instances needs to be created at the compile time only. Some of the types of master instances are UDS (Unix Domain Sockets), V4/V6 IDS (Internet Domain Sockets). UDS types of Masters are used for intra-communication and IDS can be used for both inter and intra system communication. Depending on the Communication types needed by the client, connection need to be setup between the client and the Master instances using the Communication Manager Protocols.

All the Master instances of the same type share all the global queues like protocol queue etc. Same type of Master instances are used to share the load, by mapping the UIDs to the Master instances of the same type. For example, if two UDS Masters are created, one Master can be responsible for serving static UIDs and other Master instances for all Dynamic UIDs. Even a set of specific static UIDs can be mapped to a Master instance.

**Load Sharing using same type Master-instance:**

The same type of Master instances can be created to share the load of communication. Let’s take the example of UDS Master type. A system can have “N” number of same type of Masters. There is always a default UDS/IDS Master. All the clients connect to the default at first. The Master will respond the client saying who will start serving it. In most of the cases, when the number of UIDs and load is less, the Default Master always servers the client. In case, Communication Manager feels that the Default is going to be overloaded in future, for the next new client, the Default Master will ask the client to talk to a different UDS Master. The default UDS Master will also send the ID of that Master. The client now needs to close the communication with the Default immediately and create a connection with the new Master. The Communication Manager library knows how to interpret the ID that the default Master has sent. So that for the client, create/send/receive library calls are exactly same for all Masters.

**<Future feature>**

IDS is mainly used for inter-system communication. The IDS has a sender/receiver role. When a client wants to send a message to a client in another system, it sends the message first to the IDS on the same system. The IDS now sends this message to the IDS receiver on the other system, which in turn will deliver the message to the dest client. There is a different protocol between the IDS of the different systems for reliable connection

**Communication Manager Overlay Protocols:**

Communication Manager allows to implement custom overlay protocol messaging on top of it. One such fine example is SCOM.

**System Messages:**

These are special messages sent only by the infra modules to other infra modules or user apps. These are usually high priority messages on which the recipients have to usually take actions. One example of system messages is, which sent by the Communication Manager to throttle the sending frequency.

Format of system messages:

[Msg\_type:<System message>] [submsg\_type: <Module/Functionality>] [Payload:<Msg-Id>, <Optional Message>]

The message IDs will be specific for a Module/Functionality.

**SCOM**

“SCOM” (Smart Communication) uses Communication Managers Custom Overlay Protocol. SCOM will provide library APIs to communicate with other subsystems.

The SCOM messages will consists of a header and a payload. Sometimes the payload can be optional. The header will include some of the fields like source address, destination address, payload length, message type etc

The source and destination addresses are allocated for each and every process in the system either statically or dynamically. The addresses of all the non-user modules are allocated by the system manager statically. The addresses of all the user apps are allocated by the app manager dynamically (So to add a new user app, the app manager need not to be restarted. The new user app will send SCOM messages to app\_manager trying to register itself with the system. The app\_manager then will allocate it an address and broadcast all the user apps with an updated list of addresses of user apps)

**Event Management**

<https://stackoverflow.com/questions/2533284/are-posix-pipes-lightweight>

<http://man7.org/linux/man-pages/man2/eventfd.2.html>

<https://stackoverflow.com/questions/13587003/select-doesnt-behave-properly-with-an-eventfd>

### Database Manager

### App manager

### Users Manager

## Security

# Quick Startup Guide

- Download the image “smarthome” from the dockerhub to a Linux machine.

- Spwan a container and expose the port 8080 to one of the ports on the Host machine.

*docker run -dit -p 8888:8080 --rm --name=SmartHome pruthwinkg/dockerhub-pruthwinkg:smarthome*

- Set up the “Port Forwarding” rule on the home router to allow the external requests to the Smart Home system.

# Resources

<https://www.tutorialspoint.com/postgresql/postgresql_c_cpp.htm>

<https://www.tutorialspoint.com/postgresql/postgresql_java.htm>

<https://docs.docker.com/engine/reference/commandline/docker/>

<https://gist.github.com/Alexey-N-Chernyshov/4634731>